{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["A级防火门"],"not_rendered":{"external_links":1,"defined_names":3,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"A级防火门","index":0,"n_rows":231,"n_cols":38,"rows_kept":231,"merged":[[0,0,0,32],[231,0,231,32]],"flags":["formulas_cached_only"]}
["“世纪梦想”游轮 A级防火门清单（2025-6-27）"]
["序号","甲板名称","装饰部编号","（设计院）\n门编号","门位置","防火级别","（设计院）\n门名称","HBM防火门型号","HBM图号","HBM防火门名称","订货清单/\n门开向","通孔宽(Wc)","通孔高(Hc)","钢壁开孔宽","钢壁开孔高","结构门槛高","HBM底部门框高度","门框厚度(HBM按意见全部调整为了90厚)","HBM门框样式","门框色卡","门扇色卡（内）","门扇色卡（外）","锁型","锁把高度","使用开向","闭门器","门框特殊要求","消防通道","气窗","圆气窗直径","数量（套）","备注","备注一","单价","现场做门框改做整体门框","贴防火门价格","小计","合计"]
[1,"-1F/底舱","A/-1F/001","D03","餐梯FR59","A-0","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO","950","1000","1050","1100","50","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[2,"-1F/底舱","A/-1F/002","D03","餐梯FR59","A-0","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO","950","1000","1050","1100","50","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[3,"-1F/底舱","A/-1F/003","D03","餐梯FR59","A-0","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO","950","1000","1050","1100","50","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[4,"-1F/底舱","A/-1F/004","D03","餐梯FR59","A-0","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO","950","1000","1050","1100","50","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[5,"-1F/底舱","A/-1F/005","D03","餐梯FR59","A-0","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO","950","1000","1050","1100","50","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[6,"-1F/底舱","A/-1F/006","D04","新风室FR191","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI","600","2100","700","2200","0","46.5","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","960","RI",{"$nulls":5},1]
[7,"-1F/底舱","A/-1F/007","D05","通道门FR197(直饮水间）","A-0","单扇风雨密气密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO","900","2100","1000","2200",50,"46.5","90","Z","RAL7006","RAL9016","RAL9016","C-1（沪江）","1000","RO",{"$nulls":5},1,"防火门"]
[8,"-1F/底舱","A/-1F/008","D05a","冰机室FR72","-","船用钢制隔音阻气门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RI","600","1800","700","1900","200","46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RI",{"$nulls":5},1]
[9,"-1F/底舱","A/-1F/009","D08","电缆井FR59","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO","600","1800",700,"1900","200","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[10,"-1F/底舱","A/-1F/010","D09","设备间FR73","-","船用钢制隔音阻气门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO","600","1800","700","1900","200","46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1]
[11,"-1F/底舱","A/-1F/011","D10","网络设备间FR87(左舷)","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI","800","1950","900","2050","100","46.5","90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[12,"-1F/底舱","A/-1F/012","D16","船员餐梯FR137","A-0","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO","850","1000","950","1100","900","46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","450","LO/RO",{"$nulls":5},1,"防火门"]
[13,"-1F/底舱","A/-1F/013","D17","污水处理舱 FR132（左舷）","-","钢质隔音阻气门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RI","600","1800","700","1900","200","46.5","90","A1","RAL7006","HNP-20","HNP-20","C-1（沪江）","760","RI",{"$nulls":5},1,null,"HBM制造开向LO"]
[14,"-1F/底舱","A/-1F/014","D19","音控室FR91（右舷）","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI","800","1950","900","2050","0","46.5","90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[15,"1F/主甲板","A-1F-001","D07","监控室FR158右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI","700","1950","800","2000","0","15","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[16,"1F/主甲板","A-1F-002","D06a","电缆井FR59","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",600,1700,700,1800,200,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[17,"1F/主甲板","A-1F-003","D06","电缆井FR198","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",600,1700,700,1800,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[18,"1F/主甲板","A-1F-004","D10","舵机舱FR8（左舷）","A-0","单扇风雨密气密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1,"防火门"]
[19,"1F/主甲板","A-1F-005","D11","舵机舱FR8（右舷）","A-0","单扇风雨密气密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[20,"1F/主甲板","A-1F-006","D12","机舱通道门(内)FR20（右舷）","A-60","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",700,1650,900,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[21,"1F/主甲板","A-1F-007","D13","机舱通道门(内)FR20（左舷）","A-60","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",700,1650,900,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1,"防火门"]
[22,"1F/主甲板","A-1F-008","D14","通道门FR57左舷","A-60","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(改制取消胶条下槛)（外开）","RO",850,1800,950,1900,50,"30.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","910","RO",{"$nulls":5},1,"防火门"]
[23,"1F/主甲板","A-1F-009","D15","通道门FR132（右舷）","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1,"防火门"]
[24,"1F/主甲板","A-1F-010","D15","通道门FR157右舷通道","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1,"防火门"]
[25,"1F/主甲板","A-1F-011","D15","通道门FR196左舷通道","A-30","防火风雨密门（总计与设计院清单少1扇）","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1,"防火门"]
[26,"1F/主甲板","A-1F-012","D16","通道门FR132（左舷）","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[27,"1F/主甲板","A-1F-013","D16","通道门FR77左","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[28,"1F/主甲板","A-1F-014","D16","FR197右舷通道门","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[29,"1F/主甲板","A-1F-015","D16","FR62右舷楼梯间","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[30,"1F/主甲板","A-1F-016","D16","FR193号左舷通道","A-30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1750,1000,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1,"防火门"]
[31,"1F/主甲板","A-1F-017","D17","回风室 FR122（左舷）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[32,"1F/主甲板","A-1F-018","D17","设备间 FR56左舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[33,"1F/主甲板","A-1F-019","D17a","设备间 FR52左舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[34,"1F/主甲板","A-1F-020","D18","回风室FR121右舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[35,"1F/主甲板","A-1F-021","D18","回风室FR90右舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[36,"1F/主甲板","A-1F-022","D19","通道门 FR125（左舷）","A-30","双扇防火风雨门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1200,1750,1300,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B(沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[37,"1F/主甲板","A-1F-023","D19","通道门 FR125（右舷）","A-30","双扇防火风雨门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1200,1750,1300,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B(沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[38,"1F/主甲板","A-1F-024","D19","通道门 FR136（左舷）","A-30","双扇防火风雨门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1200,1750,1300,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B(沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[39,"1F/主甲板","A-1F-025","D19","通道门 FR136（右舷）","A-30","双扇防火风雨门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1200,1750,1300,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B(沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[40,"1F/主甲板","A-1F-026","D20","冷盘间通道门 FR57右舷","A-15","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",800,1800,900,1900,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","910","LO",{"$nulls":5},1,"防火门"]
[41,"1F/主甲板","A-1F-027","D21","通道门 FR61（左舷）","A-30","双扇防火风雨密门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1200,1750,1300,1850,200,"46.5","90","Z","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[42,"1F/主甲板","A-1F-028","D21","通道门 FR73（右舷）","A-30","双扇防火风雨密门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1200,1750,1300,1850,200,"46.5","90","Z","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[43,"1F/主甲板","A-1F-029","D22","通道门 FR78（左舷）","A-30","双扇防火风雨密门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1400,1750,1500,1850,200,"46.5","90","Z","RAL7048","D327-82(威盛亚防火板)","RAL9016","C5-B(沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[44,"1F/主甲板","A-1F-030","D22","通道门 FR78（右舷）","A-30","双扇防火风雨密门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1400,1750,1500,1850,200,"46.5","90","Z","RAL7048","D327-82(威盛亚防火板)","RAL9016","C5-B(沪江）","785","LO/RO",{"$nulls":5},1,"防火门"]
[45,"1F/主甲板","A-1F-031","D23","自助洗衣房FR92左舷","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",800,1950,900,2050,0,"46.5","90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","965","RI",{"$nulls":5},1,"防火门"]
[46,"1F/主甲板","A-1F-032","D25","机修间 FR38（右舷）","A-60","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",600,1450,700,1550,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[47,"1F/主甲板","A-1F-033","D26","备件间 FR38（左舷）","A-60","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",600,1450,700,1550,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[48,"1F/主甲板","A-1F-034","D27","布草电梯FR200右舷","A-0","双扇防火装饰门","SMA15CX","Q/HN035.075","A-15级箱框双开防火门(低下槛)（内开）","LO/RO",950,1000,1050,1100,0,"15","90","A2","RAL9016","RAL9016","RAL9016","C-1（沪江）","500","LO/RO",{"$nulls":5},1,"防火门","HBM制造开向RI/LI"]
[49,"1F/主甲板","A-1F-035","D29","新风室FR130右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","965","RI",{"$nulls":5},1]
[50,"1F/主甲板","A-1F-036","D29b","新风室FR190右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","965","RI",{"$nulls":5},1]
[51,"1F/主甲板","A-1F-037","D29a","配电间FR155","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[52,"1F/主甲板","A-1F-038","D30","餐梯FR59","A-15","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[53,"1F/主甲板","A-1F-039","D30","餐梯FR59","A-15","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[54,"1F/主甲板","A-1F-040","D30","餐梯FR59","A-15","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[55,"1F/主甲板","A-1F-041","D30","餐梯FR59","A-15","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","650","LO/RO",{"$nulls":5},1,"防火门"]
[56,"1F/主甲板","A-1F-042","D30","餐梯FR59","A-15","双扇防火装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","650","LO/RO",{"$nulls":5},1,"防火门"]
[57,"1F/主甲板","A-1F-044","D31","集控室 FR27","-","船用钢质隔音阻气门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",800,2050,900,2150,0,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","965","LO","有",{"$nulls":4},1]
[58,"1F/主甲板","A-1F-045","D32","变频间FR16","-","船用钢质隔音阻气门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",800,2050,900,2150,0,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","965","RO",{"$nulls":5},1]
[59,"1F/主甲板","A-1F-046","D33","机舱通道门（外）FR20（右舷）","-","船用钢质隔音阻气门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",800,1750,900,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1]
[60,"1F/主甲板","A-1F-047","D34","机舱通道门（外）FR20（左舷）","-","船用钢质隔音阻气门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",800,1750,900,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1]
[61,"1F/主甲板","A-1F-048","D37","集控室 FR45","-","船用风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO","有",{"$nulls":4},1]
[62,"1F/主甲板","A-1F-049","D38"," FR45右舷蓄电池间","-","内河船舶轻型单扇钢质门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1]
[63,"1F/主甲板","A-1F-050","D41","通道门FR123（右舷）","A-0","防火隔音装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RO",900,1900,1000,2000,0,"46.5","90","A2","RAL7006","HNP-20","HNP-20","C5-B(沪江）","965","RO",{"$nulls":5},1,"防火门","HBM制造开向RI"]
[64,"1F/主甲板","A-1F-051","D42","通道门FR123（左舷）","A-0","防火隔音装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LO",900,1900,1000,2000,0,"46.5","90","A2","RAL7006","HNP-20","HNP-20","C5-B(沪江）","965","LO",{"$nulls":5},1,"防火门","HBM制造开向LI"]
[65,"1F/主甲板","A-1F-052","D43","垃圾舱（右舷）","-","船员风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1]
[66,"1F/主甲板","A-1F-053","D43a","辅机舱通道门FR48","A30","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",700,1750,800,1850,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1,"防火门"]
[67,"1F/主甲板","A-1F-054","D44","垃圾舱（左舷）","-","船员风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1]
[68,"1F/主甲板","A-1F-055","D45","风机室FR29（左）","-","船用风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",600,1400,700,1500,350,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","635","LO",{"$nulls":5},1]
[69,"1F/主甲板","A-1F-056","D46","风机室FR29（右）","-","船用风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",600,1400,700,1500,350,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","635","RO",{"$nulls":5},1]
[70,"1F/主甲板","A-1F-057","D47","员工洗衣房FR198右舷","-","内河船舶轻型单扇钢质门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",750,1750,850,1850,200,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","760","RO",{"$nulls":5},1]
[71,"1F/主甲板","A-1F-058","D48","洗衣房FR198左舷","-","内河船舶轻型单扇钢质门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1]
[72,"1F/主甲板","A-1F-059","D48","库房FR199左舷","-","内河船舶轻型单扇钢质门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1]
[73,"1F/主甲板","A-1F-060","D50","船员餐梯FR137","A0","双扇防火风雨密门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO","850","1000",950,1100,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B(沪江）","475","LO/RO",{"$nulls":5},1,"防火门"]
[74,"1F/主甲板","A-1F-061","D51","电工间FR45","-","内河船舶轻型单扇钢质门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1]
[75,"1F/主甲板","A-1F-062","D52","机舱通道门FR9","-","船员风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",600,1550,700,1650,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1]
[76,"1F/主甲板","A-1F-063","D53","厨房配电间FR47左舷","A0","内河船舶轻型单扇钢质门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[77,"1F/主甲板","A-1F-064","D53","CO2间FR47右舷(带观察窗）","A0","内河船舶轻型单扇钢质门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":3},"1个",200,1,"防火门"]
[78,"1F/主甲板","A-1F-065","D53","充放电间FR47右舷","A0","内河船舶轻型单扇钢质门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",750,1750,850,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[79,"1F/主甲板","A-1F-066","D18","空调设备间 FR53右舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[80,"1F/主甲板","A-1F-067","D44","垃圾舱（右舷）","-","船员风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","RO",{"$nulls":5},1]
[81,"1F/主甲板","A-1F-068","D43","垃圾舱（左舷）","-","船员风雨密钢质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",700,1650,800,1750,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","785","LO",{"$nulls":5},1]
[82,"1F/主甲板","A-1F-069","D52","船员餐梯检修门FR137","A30","双扇防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",700,600,800,700,1600,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C-1（沪江）","300","LO/RO",{"$nulls":5},1,"防火门"]
[83,"2F/上甲板","A-2F-001","D03","布草电梯FR199右舷","A-0","防火双扇装饰门","SMA15CX","Q/HN035.110","A-15级箱框双开防火门(带胶条下槛)（内开）","LO/RO",950,1000,"1050","1100",0,46.5,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","525","LO/RO",{"$nulls":5},1,"防火门","HBM制造开向RI/LI"]
[84,"2F/上甲板","A-2F-002","D05","新风室FR130右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[85,"2F/上甲板","A-2F-003","D05","新风室FR190右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[86,"2F/上甲板","A-2F-004","D05a","配电室FR155","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,46.5,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[87,"2F/上甲板","A-2F-005","D08","新风室FR87","-","铝质舱室空腹门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RI",650,1900,750,2000,20,"46.5","90","A1","RAL7006","RAL9016","D327-82(威盛亚防火板)","C-1（沪江）","940","RI",{"$nulls":5},1,null,"HBM制造开向LO"]
[88,"2F/上甲板","A-2F-006","D09","商务中心FR87","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","LI",650,1900,750,2000,20,"30.5","90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","940","LI",{"$nulls":5},1,"防火门","HBM制造开向RO"]
[89,"2F/上甲板","A-2F-007","D10","储藏室 FR203（左）","-","内河船舶轻型单扇钢质门RI40","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,15,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1]
[90,"2F/上甲板","A-2F-009","D11","储藏室 FR203（右）","-","内河船舶轻型单扇钢质门RI40","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",800,1950,900,2050,0,15,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","LI",{"$nulls":5},1]
[91,"2F/上甲板","A-2F-010","D13","设备间 FR56左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",700,1700,800,1800,350,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[92,"2F/上甲板","A-2F-011","D14","通道门FR5右舷","A-0","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","RO","有",{"$nulls":4},1,"防火门"]
[93,"2F/上甲板","A-2F-012","D14a","通道门FR5左舷","A-0","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","LO","有",{"$nulls":4},1,"防火门"]
[94,"2F/上甲板","A-2F-013","D14b","通道门FR63右舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","RI",900,1950,1000,2050,20,"30.5","90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","940","RI","有",{"$nulls":4},1,"防火门"]
[95,"2F/上甲板","A-2F-014","D15","通道门 FR218左舷","-","船用风雨密单扇铝质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1900,1000,2000,100,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B(沪江）","885","RO",{"$nulls":5},1]
[96,"2F/上甲板","A-2F-015","D15","通道门 FR217中","-","船用风雨密单扇铝质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",900,1900,1000,2000,100,"46.5","90","Z","RAL7006","RAL9016","RAL9016","C-1（沪江）","885","LO",{"$nulls":5},1]
[97,"2F/上甲板","A-2F-016","D16","设备间 FR2左舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LI",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LI",{"$nulls":5},1,"防火门"]
[98,"2F/上甲板","A-2F-017","D17","设备间 FR2右舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RI",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RI",{"$nulls":5},1,"防火门"]
[99,"2F/上甲板","A-2F-018","D20","配电间 FR61左舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","LI",800,1880,900,1980,20,"30.5","90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","940","LI","有",{"$nulls":4},1,"防火门","HBM制造开向RO"]
[100,"2F/上甲板","A-2F-019","D21","配餐间FR48左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",850,2000,950,2100,80,"46.5","90","A1","304拉丝不锈钢","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","880","LI","有",{"$nulls":4},1,"防火门","HBM制造开向RO"]
[101,"2F/上甲板","A-2F-020","D21","仓库FR52右舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",800,2000,900,2100,100,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","860","LI",{"$nulls":5},1,"防火门","HBM制造开向RO"]
[102,"2F/上甲板","A-2F-021","D22","洗碗间FR49右舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RI",850,2000,950,2100,80,"46.5","90","A1","304拉丝不锈钢","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","880","RI","有",{"$nulls":4},1,"防火门","HBM制造开向LO"]
[103,"2F/上甲板","A-2F-022","D25","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[104,"2F/上甲板","A-2F-023","D25","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[105,"2F/上甲板","A-2F-024","D25","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[106,"2F/上甲板","A-2F-025","D25","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","650","LO/RO",{"$nulls":5},1,"防火门"]
[107,"2F/上甲板","A-2F-026","D25","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B(沪江）","650","LO/RO",{"$nulls":5},1,"防火门"]
[108,"2F/上甲板","A-2F-027","D29","电缆井 FR62左舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",600,1750,700,1850,200,"46.5","90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[109,"2F/上甲板","A-2F-028","D30","电缆井 FR199左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RO",600,1950,700,2050,0,"15","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[110,"2F/上甲板","A-2F-029","D32","设备间 FR53右舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",700,1850,800,1950,200,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[111,"3F/游步甲板","A-3F-001","D03","布草电梯FR200","A-0","防火双扇装饰门","SMA15CX","Q/HN035.110","A-15级箱框双开防火门(带胶条下槛)（内开）","LO/RO",950,1000,1050,1100,0,46.5,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","525","LO/RO",{"$nulls":5},1,"防火门","HBM制造开向RI/LI"]
[112,"3F/游步甲板","A-3F-002","D05","新风室FR130右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[113,"3F/游步甲板","A-3F-003","D05","新风室FR190右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[114,"3F/游步甲板","A-3F-004","D05a","配电间FR156右舷","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[115,"3F/游步甲板","A-3F-005","D06","维修间FR62左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",700,1950,800,2050,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[116,"3F/游步甲板","A-3F-006","D07","储藏室FR181左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",750,1950,850,2050,0,30,"90","A2","RAL7006","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[117,"3F/游步甲板","A-3F-007","D07a","通道门FR63右舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","RI",900,1950,1000,2050,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI","有",{"$nulls":4},1,"防火门"]
[118,"3F/游步甲板","A-3F-008","D10","通道门FR4（左）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","RO","有",{"$nulls":4},1,"防火门"]
[119,"3F/游步甲板","A-3F-009","D11","通道门FR4（右）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","LO","有",{"$nulls":4},1,"防火门"]
[120,"3F/游步甲板","A-3F-010","D17","仓库FR52右舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",800,1950,900,2050,100,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","860","LI",{"$nulls":5},1,"防火门","HBM制造开向RO"]
[121,"3F/游步甲板","A-3F-011","D20a","设备间 FR3（右舷）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO ",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO ",{"$nulls":5},1,"防火门"]
[122,"3F/游步甲板","A-3F-012","D20b","设备间 FR3（左舷）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","L0",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","L0",{"$nulls":5},1,"防火门"]
[123,"3F/游步甲板","A-3F-013","D22","配餐间FR48左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",850,2000,950,2100,80,"46.5","90","A1","拉丝不锈钢","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","880","LI","有",{"$nulls":4},1,"防火门","HBM制造开向RO"]
[124,"3F/游步甲板","A-3F-014","D22","设备间FR199左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",850,2000,950,2100,80,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","860","LI","有",{"$nulls":4},1,"防火门","HBM制造开向RO"]
[125,"3F/游步甲板","A-3F-015","D23","配餐间FR202左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RI",850,2000,950,2100,50,"30","90","A1","拉丝不锈钢","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","880","RI","有",{"$nulls":4},1,"防火门"]
[126,"3F/游步甲板","A-3F-016","D23","洗碗间FR49右舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RI",850,2000,950,2100,80,"46.5","90","A1","拉丝不锈钢","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","880","RI","有",{"$nulls":4},1,"防火门","HBM制造开向LO"]
[127,"3F/游步甲板","A-3F-017","D24","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[128,"3F/游步甲板","A-3F-018","D24","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[129,"3F/游步甲板","A-3F-019","D24","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[130,"3F/游步甲板","A-3F-020","D24","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[131,"3F/游步甲板","A-3F-021","D24","餐梯FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[132,"3F/游步甲板","A-3F-022","D25","新风室FR87右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",650,1950,750,2050,0,"30","90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[133,"3F/游步甲板","A-3F-023","D27","设备间FR53右舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",700,1950,800,2050,100,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","860","LO",{"$nulls":5},1,"防火门"]
[134,"3F/游步甲板","A-3F-024","D28","设备间FR56左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",700,1950,800,2050,100,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","860","LO",{"$nulls":5},1,"防火门"]
[135,"3F/游步甲板","A-3F-025","D30a","电缆井FR199","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RO",600,1950,700,2050,0,"46.5","90","A2","RAL7006","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门","HBM制造开向RI"]
[136,"3F/游步甲板","A-3F-026","D30","电缆井FR61","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",600,1750,700,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[137,"3F/游步甲板","A-3F-027","D31","储藏室FR110左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",800,1950,900,2050,0,15,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[138,"3F/游步甲板","A-3F-028","D31","消洗间FR112右舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","LI",800,1950,900,2050,50,"30.5","90","A1","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","910","LI",{"$nulls":5},1,"防火门","HBM制造开向LO"]
[139,"3F/游步甲板","A-3F-029","D32","储藏室FR97右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,15,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[140,"3F/游步甲板","A-3F-030","D32","消洗间FR111左舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","RI",800,1950,900,2050,50,"30.5","90","A1","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","910","RI",{"$nulls":5},1,"防火门","HBM制造开向RO"]
[141,"3F/游步甲板","A-3F-031","D32","储藏室FR110右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,15,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[142,"3F/游步甲板","A-3F-032","/","FR87检修门","A-60","A60级单扇防火检修门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加，单面把手"]
[143,"3F/游步甲板","A-3F-033","/","餐梯检修门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",700,600,800,700,1600,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","350","LO/RO",{"$nulls":5},1,"防火门"]
[144,"4F/娱乐甲板","A-4F-001","D03a","布草电梯FR200","A-0","防火双扇装饰门","SMA15CX","Q/HN035.075","A-15级箱框双开防火门(低下槛)（内开）","LO/RO",950,1000,1050,1100,0,30,"90","A2","RAL7006","RAL9016","W3397(万美国产定制防火板)","C-1（沪江）","525","LO/RO",{"$nulls":5},1,"防火门","HBM制造开向RI/LI"]
[145,"4F/娱乐甲板","A-4F-002","D05","新风室FR130右舷","-","船用钢质隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1950,700,2050,0,"46.5","90","A2","RAL7006","RAL9016","W3397(万美国产定制防火板)","C-1（沪江）","965","RI",{"$nulls":5},1]
[146,"4F/娱乐甲板","A-4F-003","D05","新风室FR190右舷","-","船用钢质隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1950,700,2050,0,"46.5","90","A2","RAL7006","RAL9016","W3397(万美国产定制防火板)","C-1（沪江）","965","RI",{"$nulls":5},1]
[147,"4F/娱乐甲板","A-4F-004","D05a","配电间FR155","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1950,700,2050,0,"46.5","90","A2","RAL7006","RAL9016","W3397(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[148,"4F/娱乐甲板","A-4F-005","D06a","设备间FR62左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",700,1950,800,2050,0,"30","90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门","和设计院沟通增加"]
[149,"4F/娱乐甲板","A-4F-006","D08a","设备间 FR3右舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO ",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO ",{"$nulls":5},1,"防火门"]
[150,"4F/娱乐甲板","A-4F-007","D08b","设备间 FR3左舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","L0",700,1750,800,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","L0",{"$nulls":5},1,"防火门"]
[151,"4F/娱乐甲板","A-4F-008","D11","通道门 FR3左舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","RO","有",{"$nulls":4},1,"防火门"]
[152,"4F/娱乐甲板","A-4F-009","D11a","通道门 FR77左舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LI",900,1900,1000,2000,100,"46.5","90","A1","RAL7048","RAL9016","D327-82(威盛亚防火板)","C-1（沪江）","860","LI",{"$nulls":5},1,"防火门"]
[153,"4F/娱乐甲板","A-4F-010","D12","通道门 FR3右舷","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","LI",{"$nulls":5},1,"防火门","HBM制造开向RO"]
[154,"4F/娱乐甲板","A-4F-011","D14a","配电间 FR62","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",700,1950,800,2050,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[155,"4F/娱乐甲板","A-4F-012","D15","配餐间FR49左舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",850,2100,950,2100,80,"46.5","90","A1","304拉丝不锈钢","S185-07(威盛亚防火板)","S185-07(威盛亚防火板)","C-1（沪江）","880","LI","有",{"$nulls":4},1,"防火门","HBM制造开向RO"]
[156,"4F/娱乐甲板","A-4F-013","D15","洗碗间FR48右舷","A-15","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LI",850,2100,950,2100,80,"46.5","90","A1","304拉丝不锈钢","S185-07(威盛亚防火板)","S185-07(威盛亚防火板)","C-1（沪江）","880","LI","有",{"$nulls":4},1,"防火门","HBM制造开向RO"]
[157,"4F/娱乐甲板","A-4F-014","D16","餐梯门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[158,"4F/娱乐甲板","A-4F-015","D16","餐梯门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[159,"4F/娱乐甲板","A-4F-016","D16","餐梯门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[160,"4F/娱乐甲板","A-4F-017","D16","餐梯门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[161,"4F/娱乐甲板","A-4F-018","D22a","通道门 FR207（右舷）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（外开）","LO",900,1950,1000,2050,0,"30","90","A1","RAL7006","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","985","LO",{"$nulls":5},1,"防火门"]
[162,"4F/娱乐甲板","A-4F-019","D22b","通道门 FR207（左舷）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（外开）","RO",900,1950,1000,2050,0,"30","90","A1","RAL7006","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","985","RO",{"$nulls":5},1,"防火门"]
[163,"4F/娱乐甲板","A-4F-020","D23","设备间 FR52左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RO",650,2000,750,2100,0,15,"90","A2","RAL9016","RAL9016","RAL9016","C-1（沪江）","985","RO",{"$nulls":5},1,"防火门","HBM制造开向LI"]
[164,"4F/娱乐甲板","A-4F-021","D24","设备间 FR52右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LO",650,2000,750,2100,0,15,"90","A2","RAL9016","RAL9016","RAL9016","C-1（沪江）","985","LO",{"$nulls":5},1,"防火门","HBM制造开向RI"]
[165,"4F/娱乐甲板","A-4F-022","D29","电缆井FR61","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",600,1750,700,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1,"防火门"]
[166,"4F/娱乐甲板","A-4F-023","D29","电缆井FR199","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RO",600,1950,700,2050,0,30,"90","A2","RAL7006","RAL9016","W3397(万美国产定制防火板)","C-1（沪江）","985","RO",{"$nulls":5},1,"防火门","HBM制造开向LI"]
[167,"4F/娱乐甲板","A-4F-024","D30","储藏室 FR125(左）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[168,"4F/娱乐甲板","A-4F-025","D31","储藏室 FR125（右）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[169,"4F/娱乐甲板","A-4F-026","D36","库房 FR48右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",750,2000,850,2100,0,30,"90","A2","RAL8019","8848 NT(富美家防火板)","8848 NT(富美家防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[170,"4F/娱乐甲板","A-4F-027","D36","库房 FR149右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[171,"4F/娱乐甲板","A-4F-028","D36","库房 FR187右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3397(万美国产定制防火板)","W3397(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[172,"4F/娱乐甲板","A-4F-029","D37","库房 FR48左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",750,2000,850,2100,0,30,"90","A2","RAL8019","8848 NT(富美家防火板)","8848 NT(富美家防火板)","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[173,"4F/娱乐甲板","A-4F-030","D37a","楼梯通道门 FR62","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","RI",900,1950,1000,2050,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI","有",{"$nulls":4},1,"防火门"]
[174,"4F/娱乐甲板","A-4F-031","/","卫生间检修门","A-60","A60级单扇防火检修门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加"]
[175,"4F/娱乐甲板","A-4F-032","/","卫生间检修门","A-60","A60级单扇防火检修门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加"]
[176,"5F/驾驶甲板","A-5F-001","D05","配电间FR156右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",600,1950,700,2050,0,30,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[177,"5F/驾驶甲板","A-5F-002","D05a","新风室FR130右舷","-","船用钢质隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[178,"5F/驾驶甲板","A-5F-003","D05a","新风室FR190右舷","-","船用钢质隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,"46.5","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[179,"5F/驾驶甲板","A-5F-004","D06","设备间FR63左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",700,1950,800,2050,0,"30","90","A2","RAL7048","S185-07(威盛亚防火板)","S185-07(威盛亚防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[180,"5F/驾驶甲板","A-5F-005","D06","设备间FR57右舷","A-0","防火装饰门（新增）","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",700,1950,800,2050,0,"30","90","A2","RAL8028","9365G (富美家）","9365G (富美家）","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[181,"5F/驾驶甲板","A-5F-006","D06a","设备间FR52左舷","A-0","防火装饰门（新增）","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",700,1950,800,2050,0,"30","90","A2","RAL8028","9365G (富美家）","9365G (富美家）","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[182,"5F/驾驶甲板","A-5F-007","D08a","设备间 FR6（左舷）","-","铝质舱室空腹门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RO",700,1850,800,1950,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","RO",{"$nulls":5},1]
[183,"5F/驾驶甲板","A-5F-008","D08b","设备间 FR6（右舷）","-","铝质舱室空腹门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LO",700,1850,800,1950,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1]
[184,"5F/驾驶甲板","A-5F-009","D11","通道门 FR6（左）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","RO","有",{"$nulls":4},1,"防火门"]
[185,"5F/驾驶甲板","A-5F-010","D12","通道门 FR6（右）","A-30","防火装饰门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","LO",900,1950,1000,2050,100,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","860","LO","有",{"$nulls":4},1,"防火门"]
[186,"5F/驾驶甲板","A-5F-011","D14","布草电梯FR199","A-0","防火双扇装饰门","SMA15CX","Q/HN035.075","A-15级箱框双开防火门(低下槛)（内开）","LO/RO",950,1000,1050,1100,0,"30","90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","525","LO/RO",{"$nulls":5},1,"防火门","HBM制造开向LI/RI"]
[187,"5F/驾驶甲板","A-5F-012","D15","餐梯门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[188,"5F/驾驶甲板","A-5F-013","D15","餐梯门FR57","A-60","防火双扇装饰门","SMA60CX","Q/HN035.039","A-60级箱框双开防火门(带胶条下槛)（外开）","LO/RO",900,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C5-B（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[189,"5F/驾驶甲板","A-5F-014","D16a","库房FR59右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",750,1900,850,2000,0,"30","90","A2","RAL8019","S185-07(威盛亚防火板)","S185-07(威盛亚防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[190,"5F/驾驶甲板","A-5F-015","D16a","通道门FR63右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(改制取消胶条下槛)（外开）","LI",900,1950,1000,2050,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[191,"5F/驾驶甲板","A-5F-016","D17","配电间FR62左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",700,1900,800,2000,0,"30","90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","RI","有",{"$nulls":4},1,"防火门"]
[192,"5F/驾驶甲板","A-5F-017","D29","驾驶室 FR212","A-15","A15级箱框防火门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",900,1900,1000,2000,0,"15","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","985","RI","有",{"$nulls":4},1,"防火门"]
[193,"5F/驾驶甲板","A-5F-018","D30","驾驶室 FR212","A-15","A15级箱框防火门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",900,1900,1000,2000,0,"15","90","A2","RAL7006","HNP-20","HNP-20","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[194,"5F/驾驶甲板","A-5F-019","D33","电缆井FR200","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RO",600,1950,700,2050,0,"30","90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","985","RO",{"$nulls":5},1,"防火门","HBM制造开向LI"]
[195,"5F/驾驶甲板","A-5F-020","D33a","电缆井FR61左舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",600,1750,700,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[196,"5F/驾驶甲板","A-5F-023","D36","储藏室FR110左舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[197,"5F/驾驶甲板","A-5F-024","D36","消洗间FR112右舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","LI",800,1900,900,2000,50,"30.5","90","A1","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","910","LI",{"$nulls":5},1,"防火门","HBM制造开向LO"]
[198,"5F/驾驶甲板","A-5F-025","D37","消洗间FR112左舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(改制取消胶条下槛)（外开）","RI",800,1900,900,2000,50,30.5,"90","A1","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","910","RI",{"$nulls":5},1,"防火门"]
[199,"5F/驾驶甲板","A-5F-026","D37","储藏室FR110右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,"30","90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门","HBM制造开向RO"]
[200,"5F/驾驶甲板","A-5F-027","D38","工作间FR98右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[201,"5F/驾驶甲板","A-5F-028","/","布草电梯检修门FR199","A-0","防火双扇装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",700,600,800,700,null,"46.5","90","A1","304拉丝不锈钢","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","350","LO/RO",{"$nulls":5},1,"防火门"]
[202,"5F/驾驶甲板","A-5F-029","/","卫生间检修门","A-60","A60级单扇防火检修门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加"]
[203,"5F/驾驶甲板","A-5F-030","/","卫生间检修门","A-60","A60级单扇防火检修门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加"]
[204,"6F/阳光甲板","A-6F-001","D03a","餐梯FR59","A-0","防火双扇装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[205,"6F/阳光甲板","A-6F-002","D03a","餐梯FR59","A-0","防火双扇装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",950,1000,1050,1100,50,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","500","LO/RO",{"$nulls":5},1,"防火门"]
[206,"6F/阳光甲板","A-6F-003","D05","电缆井 FR199","A-0","防火风雨密门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","RO",600,1100,700,1200,350,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","550","LO","有",{"$nulls":4},1,"防火门"]
[207,"6F/阳光甲板","A-6F-004","D06","设备间FR79右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",750,1900,850,2000,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[208,"6F/阳光甲板","A-6F-005","D06","设备间FR62左舷","A-0","防火装饰门","MA15CX","Q/HN035.071","A-15级箱框防火门(低下槛)（外开）","LI",700,1950,800,2050,0,30,"90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[209,"6F/阳光甲板","A-6F-006","D06a","工作间FR63左舷","A-0","防火装饰门","MA15CX","Q/HN035.071","A-15级箱框防火门(低下槛)（外开）","RI",700,1950,800,2050,0,30,"90","A1","304拉丝不锈钢","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C5-B（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[210,"6F/阳光甲板","A-6F-007","D07a","工作间FR59右舷","A-0","防火装饰门","MA15CX","Q/HN035.071","A-15级箱框防火门(低下槛)（外开）","LI",700,1950,800,2050,0,30,"90","A1","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C5-B（沪江）","500","LI",{"$nulls":5},1,"防火门"]
[211,"6F/阳光甲板","A-6F-008","D08","新风室FR130右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LI",600,1900,700,2000,0,46.5,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","LI",{"$nulls":5},1]
[212,"6F/阳光甲板","A-6F-009","D08","新风室FR190右舷","-","船用钢制隔音阻气门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,46.5,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","965","RI",{"$nulls":5},1]
[213,"6F/阳光甲板","A-6F-010","D15","配电间FR156右舷","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RI",600,1900,700,2000,0,46.5,"90","A2","RAL7006","FX3001-811（天利百晟）","FX3001-811（天利百晟）","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[214,"6F/阳光甲板","A-6F-011","D18","储藏室 FR110（左舷）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","LI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","LI",{"$nulls":5},1,"防火门"]
[215,"6F/阳光甲板","A-6F-012","D19","储藏室 FR110（右舷）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI",{"$nulls":5},1,"防火门"]
[216,"6F/阳光甲板","A-6F-013","D19","工作间 FR98（右舷）","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(低下槛)（内开）","RI",800,1950,900,2050,0,30,"90","A2","304拉丝不锈钢","W3396(万美国产定制防火板)","W3396(万美国产定制防火板)","C-1（沪江）","985","RI","有",{"$nulls":4},1,"防火门"]
[217,"6F/阳光甲板","A-6F-014","D20","楼梯间FR164右舷","-","风雨密单扇铝质门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","RO",900,1850,1000,1950,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B（沪江）","760","RO","有",{"$nulls":4},1]
[218,"6F/阳光甲板","A-6F-015","D21","商场通道门FR63（左)","-","风雨密双扇铝质门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1400,1850,1500,1950,100,"46.5","90","Z","RAL7048","D327-82(威盛亚防火板)","RAL9016","C-1（沪江）","885","LO/RO",{"$nulls":5},1]
[219,"6F/阳光甲板","A-6F-016","D21","商场通道门FR63(右）","-","风雨密双扇铝质门","SZMA60CG-FYQM","Q262LSBZ1202","SZMA60CG-FYQM型双开防风雨防火门","LO/RO",1400,1850,1500,1950,100,"46.5","90","Z","RAL7048","D327-82(威盛亚防火板)","RAL9016","C-1（沪江）","885","LO/RO",{"$nulls":5},1]
[220,"6F/阳光甲板","A-6F-017","D25a","通道门FR63右舷","A-0","防火装饰门","MA15CX","Q/HN035.072","A-15级箱框防火门(改制取消胶条下槛)（外开）","LI",900,1950,1000,2050,0,30,"90","A2","RAL7048","D327-82(威盛亚防火板)","D327-82(威盛亚防火板)","C-1（沪江）","985","LI","有",{"$nulls":4},1,"防火门"]
[221,"6F/阳光甲板","A-6F-018","D27","电缆井FR62左舷","A-0","防火装饰门","MA15CX","Q/HN035.106","A-15级箱框防火门(带胶条下槛)（外开）","LO",600,1750,700,1850,200,"46.5","90","A1","RAL9016","RAL9016","RAL9016","C-1（沪江）","760","LO",{"$nulls":5},1,"防火门"]
[222,"6F/阳光甲板","A-6F-019","D27","风机室 FR82（左）","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","LO",600,1900,700,2000,0,46.5,"90","A2","RAL7048","RAL9016","D327-82(威盛亚防火板)","C-1（沪江）","985","LO",{"$nulls":5},1,"防火门","HBM制造开向RI"]
[223,"6F/阳光甲板","A-6F-020","D29","风机室 FR82（右）","A-0","防火装饰门","MA15CX","Q/HN035.107","A-15级箱框防火门(带胶条下槛)（内开）","RO",600,1900,700,2000,0,46.5,"90","A2","RAL7048","RAL9016","D327-82(威盛亚防火板)","C-1（沪江）","985","RO",{"$nulls":5},1,"防火门","HBM制造开向LI"]
[224,"6F/阳光甲板","A-6F-021","D05","楼梯间FR199","A-0","防火风雨密门","ZMA60CG-FYQM","Q262LSBZ1201","ZMA60CG-FYQM型单开防风雨防火门","LO",900,1850,1000,1950,200,"46.5","90","Z","RAL9016","RAL9016","RAL9016","C5-B（沪江）","760","LO","有",{"$nulls":4},1,"防火门"]
[225,"6F/阳光甲板","A-6F-022","/","卫生间检修门（右）","A-60","A60级单扇防火门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加"]
[226,"6F/阳光甲板","A-6F-023","/","卫生间检修门（左）","A-60","A60级单扇防火门","MA60CX","Q/HN035.036","A-60级箱框防火门(带胶条下槛)（外开）","RO","450","1200",550,1300,"250","46.5","90","A1","RAL9016","RAL9016","RAL9016","C5-F（沪江）","600","RO",{"$nulls":5},1,"防火门","参照绿洲增加"]
[227,"6F/阳光甲板","A-6F-024","D06","餐梯检修门FR59","A-0","防火双扇装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",700,700,800,800,1600,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","350","LO/RO",{"$nulls":5},1,"防火门"]
[228,"6F/阳光甲板","A-6F-025","D06","餐梯检修门FR59","A-0","防火双扇装饰门","SMA15CX","Q/HN035.109","A-15级箱框双开防火门(带胶条下槛)（外开）","LO/RO",700,700,800,800,1600,"46.5","90","A1","304拉丝不锈钢","304哑光不锈钢","304哑光不锈钢","C-1（沪江）","350","LO/RO",{"$nulls":5},1,"防火门"]
[{"$nulls":15},"总计",{"$nulls":14},228]